#### Served with love!

With our cookies we would like to offer you the best shopping experience possible with everything that goes with it. This includes, for example, suitable offers, personalized ads and remembering preferences. If this is okay with you, simply agree to the use of cookies for preferences, statistics and marketing by clicking on "Alright!" (show all).
You can withdraw your consent at anytime via the cookie settings (here)
Imprint · Privacy Policy
To the page content

- Products
- Service
- About Us

Customer Centre login
Country and Language
Energy Efficiency Class

# Litecraft

Litecraft WashX.432 sw
1

- Colour temperature adjustable from 3000 - 6000 K
- Beam angle: 120°
- Colour: Temperature macros preprogrammed

Litecraft WashX.21

- Homogeneous wash effect
- Saturated colours and pastel shades
- Control via DMX512

Litecraft BeamX.7
6

- Light source: 7-Piece multicolour LEDs in red, green, blue and white
- Beam angle: 10° (25° frost filter included)
- Control: DMX (2/3/4/5/10 channels), Master/Slave, automatic programs, fixed colours

Litecraft HELD SLNT WW Profile
Litecraft HELD SLNT WW Profile; 130W COB LED profile spotlight (base without lens tube); Thanks to the specially developed cooling system, forced cool...
Litecraft HELD Zoom Tube 25°-50°
Litecraft HELD Zoom Tube 25°-50°; 25-50° zoom lens tube; Continuous zoom; Fits both the Held SLNT WW and the Held FCL; Includes color filter frame; Di...
Litecraft BeamX.7 IP
5

- Rainproof housing
- Light source: 7 Pieces of multicolour LEDs in the colours red, green, blue and white
- Beam angle: 10°

Litecraft Mirrorball Safety
6

- According to BGV C1
- Max load: 80 kg
- For 12-fold safety

Litecraft Truss PA Tower

- can be employed for both indoor and outdoor use
- Only two people required for setup
- does not require a Sleeveblock

Litecraft PowerBarX.15 IP65 RGBW
1

- Single-pixel control for pixel mapping
- Selectable dimmer curves
- Flicker free

Litecraft PowerBarX.15 IP65 RGBW B-Stock
B-Stock, Litecraft PowerBarX.15 IP65 RGBW, professional light bar with 15 RGBW multi-chip LEDs, single-pixel control for pixel mapping, selectable dim...
Litecraft WashXTC

- 32 RGBW x-in-1 LEDs
- Homogeneous wash
- Saturated colours and pastel shades

Litecraft SUP Stand Up Plate

- With Omega quick-release fasteners and mini TV spigot 16 mm mount
- Suitable for LITECRAFT and ELATION spotlights and many other manufacturers
- Enables quick and easy conversion for use on the base of all ...

Litecraft BeamX.12

- 12x RGBW multi-chip LEDs
- Beam angle: 10° (frost filter 20°)
- Pre-programmed colour programmes

Free Shipping Over £149
The prices shown include VAT.
Need help?